**19” 24 port module carrier 1 HU, grey**

Module carrier made of metal for 19” rack mount;

panel accepts a minimum of 24 RJ45 couplers and modules;

ports labeled 1 to 24 on panel;

comes with 24 unshielded RJ45 couplers Cat.6 with jacks on the front and the rear, for applications according to ISO/IEC 11801-1 1Gbit/s, PoE+;

optimized contact design to avoid sparcs in the area of data transmission;

The channel consisting of this coupler and the connectorized cable as specified elsewhere in this tender has to meet or exceed the specifications of ISO/IEC 11801-1 channel class E;

**Features:**

RJ45 coupler

Depth: ≤ 29.8 mm

Width: ≤ 17.0 mm

Performance: for ISO/IEC 11801-1 class E

Shielding: unshielded

Plug compatibility: RJ45, RJ12 and RJ11 plugs,

protection against over-

bending the contacts

Mating cycles: ≥ 750

Cable diameter: ≤ 9 mm

Contacts: 8

...Wiring scheme: 1:1

Contact design: Optimized design, evidence

provided by data sheet

Module carrier:

Depth: ≤ 28 mm

Material: sheet steel, powder coated

Color: light grey like RAL 7035

Number of ports: ≥ 24

Number of cable ties: ≥ 24

Manufacturer: Telegärtner

Type: 19“ module carrier 1U

Part No.: 100007008