Installation cable S/FTP 4x2xAWG23/1, C.7, PUR - F

Installation cable S/FTP 4x2xAWG23/1, for EN 50173 and ISO/IEC 11802 class F links or higher;

meets the specifications of EN 50288-4-1;

cable jacket made of oil-resistant polyurethane;

reaction to fire class Fca or better according to European CPR;

fire retardant according to ISO/IEC 60332-1;

segregation classification “d” of EN 50174-2:2018-10;

Fire load: ≤ 0.33 kWh/m;

Cable outer diameter: ≤ 7.5 mm;

Colour of cable jacket: green;

Manufacturer: Telegärtner

Type: STX 900

Part No.: L02002A0143