Installation cable S/FTP 4x2xAWG23/1, C.7, PE - F

Installation cable S/FTP 4x2xAWG23/1, for EN 50173 and ISO/IEC 11801 class F links or higher;

meets the specifications of EN 50288-4-1;

cable jacket made of UV-resistant polyethylene;

reaction to fire class Fca or better according to European CPR;

fire retardant according to ISO/IEC 60332-1;

segregation classification “d” of EN 50174-2:2018-10;

Cable outer diameter: ≤ 8.0 mm;

Colour of cable jacket: black;

Manufacturer: Telegärtner

Type: AMJ 1000

Part No.: L02002A0146